Strain gauge test output for Beam 4 ( 4 (2-Mid / 2-Right) Expantion Anchors - Hex Head 3/8") |  |  |
Anchors Tighten Strength | Strain No. | Strain Location | CH. No. | Test No. | Test Results (u) | Avrg.
No load from the 2 new right side anchors | 1 | Top Face - Right | 0 | 1st | -3.9927 | -3.83
No load from the 2 new right side anchors | 1 | Top Face - Right | 0 | 2nd | -3.8034 |
No load from the 2 new right side anchors | 1 | Top Face - Right | 0 | 3rd | -3.6947 |
No load from the 2 new right side anchors | 2 | Top Face - Left | 3 | 1st | -27.8417 | -27.70
No load from the 2 new right side anchors | 2 | Top Face - Left | 3 | 2nd | -28.4028 |
No load from the 2 new right side anchors | 2 | Top Face - Left | 3 | 3rd | -26.8702 |
No load from the 2 new right side anchors | 3 | Side Fcae - Top | 4 | 1st | 39.34 | 38.92
No load from the 2 new right side anchors | 3 | Side Fcae - Top | 4 | 2nd | 37.9052 |
No load from the 2 new right side anchors | 3 | Side Fcae - Top | 4 | 3rd | 39.5087 |
No load from the 2 new right side anchors | 4 | Side Face - Bottom | 5 | 1st | -1.6574 | -0.64
No load from the 2 new right side anchors | 4 | Side Face - Bottom | 5 | 2nd | -1.3656 |
No load from the 2 new right side anchors | 4 | Side Face - Bottom | 5 | 3rd | 1.1092 |
1 | 1 | Top Face - Right | 0 | 1st | 1.7211 | 0.58
1 | 1 | Top Face - Right | 0 | 2nd | -1.5985 |
1 | 1 | Top Face - Right | 0 | 3rd | 1.6054 |
1 | 2 | Top Face - Left | 3 | 1st | -17.9653 | -18.81
1 | 2 | Top Face - Left | 3 | 2nd | -19.3086 |
1 | 2 | Top Face - Left | 3 | 3rd | -19.1613 |
1 | 3 | Side Fcae - Top | 4 | 1st | 40.62 | 41.00
1 | 3 | Side Fcae - Top | 4 | 2nd | 41.1404 |
1 | 3 | Side Fcae - Top | 4 | 3rd | 41.2459 |
1 | 4 | Side Face - Bottom | 5 | 1st | -2.2031 | -1.83
1 | 4 | Side Face - Bottom | 5 | 2nd | -1.4183 |
1 | 4 | Side Face - Bottom | 5 | 3rd | -1.8683 |
2 | 1 | Top Face - Right | 0 | 1st | -5.7208 | -6.44
2 | 1 | Top Face - Right | 0 | 2nd | -7.4244 |
2 | 1 | Top Face - Right | 0 | 3rd | -6.1849 |
2 | 2 | Top Face - Left | 3 | 1st | -29.3533 | -29.05
2 | 2 | Top Face - Left | 3 | 2nd | -28.6448 |
2 | 2 | Top Face - Left | 3 | 3rd | -29.1565 |
2 | 3 | Side Fcae - Top | 4 | 1st | 40.4688 | 41.29
2 | 3 | Side Fcae - Top | 4 | 2nd | 41.5096 |
2 | 3 | Side Fcae - Top | 4 | 3rd | 41.9036 |
2 | 4 | Side Face - Bottom | 5 | 1st | -2.0229 | -1.96
2 | 4 | Side Face - Bottom | 5 | 2nd | -1.8226 |
2 | 4 | Side Face - Bottom | 5 | 3rd | -2.02 |
3 | 1 | Top Face - Right | 0 | 1st | -5.0758 | -4.70
3 | 1 | Top Face - Right | 0 | 2nd | -5.4474 |
3 | 1 | Top Face - Right | 0 | 3rd | -3.5755 |
3 | 2 | Top Face - Left | 3 | 1st | -33.8669 | -33.61
3 | 2 | Top Face - Left | 3 | 2nd | -33.1339 |
3 | 2 | Top Face - Left | 3 | 3rd | -33.8283 |
3 | 3 | Side Fcae - Top | 4 | 1st | 39.449 | 39.92
3 | 3 | Side Fcae - Top | 4 | 2nd | 41.0244 |
3 | 3 | Side Fcae - Top | 4 | 3rd | 39.2977 |
3 | 4 | Side Face - Bottom | 5 | 1st | -1.8472 | -1.48
3 | 4 | Side Face - Bottom | 5 | 2nd | -1.3761 |
3 | 4 | Side Face - Bottom | 5 | 3rd | -1.2179 |