Strain gauge test output for Beam 4 ( 6 (2-Mid / 2-Right / 2-left) Expantion Anchors - Hex Head 3/8") |  |  |  |
Anchors Tighten Strength | Strain No. | Strain Location | CH. No. | Test No. | Test Results (u) | Avrg.
No load from the 2 new left side anchors | 1 | Top Face - Right | 0 | 1st | -1.8544 | -1.67
No load from the 2 new left side anchors | 1 | Top Face - Right | 0 | 2nd | -1.1954 |
No load from the 2 new left side anchors | 1 | Top Face - Right | 0 | 3rd | -1.9631 |
No load from the 2 new left side anchors | 2 | Top Face - Left | 3 | 1st | -31.1174 | -31.05
No load from the 2 new left side anchors | 2 | Top Face - Left | 3 | 2nd | -32.0643 |
No load from the 2 new left side anchors | 2 | Top Face - Left | 3 | 3rd | -29.974 |
No load from the 2 new left side anchors | 3 | Side Fcae - Top | 4 | 1st | 39.4068 | 39.41
No load from the 2 new left side anchors | 3 | Side Fcae - Top | 4 | 2nd | 39.0868 |
No load from the 2 new left side anchors | 3 | Side Fcae - Top | 4 | 3rd | 39.7479 |
No load from the 2 new left side anchors | 4 | Side Face - Bottom | 5 | 1st | -1.1406 | -0.43
No load from the 2 new left side anchors | 4 | Side Face - Bottom | 5 | 2nd | -1.3832 |
No load from the 2 new left side anchors | 4 | Side Face - Bottom | 5 | 3rd | 1.2393 |
1 | 1 | Top Face - Right | 0 | 1st | -1.1674 | -1.44
1 | 1 | Top Face - Right | 0 | 2nd | -1.4758 |
1 | 1 | Top Face - Right | 0 | 3rd | -1.684 |
1 | 2 | Top Face - Left | 3 | 1st | -31.3664 | -30.12
1 | 2 | Top Face - Left | 3 | 2nd | -29.4304 |
1 | 2 | Top Face - Left | 3 | 3rd | -29.5493 |
1 | 3 | Side Fcae - Top | 4 | 1st | 41.5624 | 42.09
1 | 3 | Side Fcae - Top | 4 | 2nd | 43.3207 |
1 | 3 | Side Fcae - Top | 4 | 3rd | 41.388 |
1 | 4 | Side Face - Bottom | 5 | 1st | -1.1336 | -1.33
1 | 4 | Side Face - Bottom | 5 | 2nd | -1.3691 |
1 | 4 | Side Face - Bottom | 5 | 3rd | -1.4839 |
2 | 1 | Top Face - Right | 0 | 1st | -10.3197 | -9.44
2 | 1 | Top Face - Right | 0 | 2nd | -9.0228 |
2 | 1 | Top Face - Right | 0 | 3rd | -8.9777 |
2 | 2 | Top Face - Left | 3 | 1st | -40.9406 | -39.22
2 | 2 | Top Face - Left | 3 | 2nd | -38.5278 |
2 | 2 | Top Face - Left | 3 | 3rd | -38.2051 |
2 | 3 | Side Fcae - Top | 4 | 1st | 44.2877 | 43.89
2 | 3 | Side Fcae - Top | 4 | 2nd | 43.3829 |
2 | 3 | Side Fcae - Top | 4 | 3rd | 44.0029 |
2 | 4 | Side Face - Bottom | 5 | 1st | -1.3093 | -1.28
2 | 4 | Side Face - Bottom | 5 | 2nd | -1.0422 |
2 | 4 | Side Face - Bottom | 5 | 3rd | -1.4992 |
3 | 1 | Top Face - Right | 0 | 1st | -10.9612 | -11.14
3 | 1 | Top Face - Right | 0 | 2nd | -10.6177 |
3 | 1 | Top Face - Right | 0 | 3rd | -11.834 |
3 | 2 | Top Face - Left | 3 | 1st | -50.6477 | -49.25
3 | 2 | Top Face - Left | 3 | 2nd | -48.8487 |
3 | 2 | Top Face - Left | 3 | 3rd | -48.2548 |
3 | 3 | Side Fcae - Top | 4 | 1st | 44.7168 | 45.10
3 | 3 | Side Fcae - Top | 4 | 2nd | 45.0227 |
3 | 3 | Side Fcae - Top | 4 | 3rd | 45.5471 |
3 | 4 | Side Face - Bottom | 5 | 1st | -2.1706 | -1.80
3 | 4 | Side Face - Bottom | 5 | 2nd | -1.2285 |
3 | 4 | Side Face - Bottom | 5 | 3rd | -1.9878 |