# guidance

The Guidance node is a ROS node is responsible for guidance state machine management and for providing a pass-through service to invoke the system enable command from the UI.

Link to detailed design document on Confluence: [Click Here](https://usdot-carma.atlassian.net/wiki/spaces/CRMPLT/pages/1309442090/Detailed+Design+-+Guidance)